**Charger Operations Procedures**

Plug Charger to forklift

Charger will automatically start the charge after 60 seconds has passed

If it does not Auto Start? Was not discussed?

If Charger starts charging it will shut down automatically when it reaches the cycle

If Unit lights are lit up to complete. Just unplug the forklift connection.

If the light is **not lit** to **complete** do not unplug if you must **hit the** **Start Stop** button first.

**Bone Crusher / Paster**

1 Always wear protective equipment Safety Glasses Hearing Protection Gloves. Visitors must also wear this.

2 Rib bones and small bones are ideal. If necessary due to lack of smaller bones cut larger bones do not just throw large bones into the grinder.

3 Ensure all latches are secured prior to starting and cover the opening to prevent bone fragments from coming out through the opening.

4 Never try to unjam **any equipment** without the lock out system being put in place. It’s there, use it.

5 Ensure Bone Paster is reassembled correctly and never put your fingers down into the funnel use a spatula to scrap the funnel not your hand.

Cleaning of both units must be partially disassembled and thoroughly cleaned using the power washer. Spray with a bit of bleach and rinse.

**Big Grinder / Mixer**

1 All guards must be in place and never operate either equipment alone.

2 Add material slowly not to jamb equipment.

3 Never lean over or into either Mixer or grinder.

4 Grinder must be dis-assembled to thoroughly clean.

5 Apply Vegetable oil to prevent rusting.

Continued Page 2

Signed:

Name (print) Title Signature Date

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |