**Building and Yard Safety**

* It is mandatory that safety boots are to be worn by all full-time personnel when behind roped area in yard.
* Safety glasses must be worn in all production areas by all personnel even in the yard, for example, grinding outside the garage.
* Safety stands are to be used when under any jacked-up equipment or materials
* Block up and use safety straps on any hydraulic device when working under it - i.e. truck box lift, truck forks and loader bucket etc.
* Use welding gloves and masks when working with torches and or welder \*Use respirator mask and/or ear protection when spray painting, welding aluminum, painting steel, weed eating or grinding etc.
* Clean up oil spills with kitty litter
* Fully open both doors for ventilation when running any type of vehicle inside the garage

Signed:

Name (print) Title Signature Date

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |