**Operating the dehydrator**

Operations needs to be sanitized and washed before dehydrating.

Dehydrator needs to be cleaned, screens must be sanitized, and power washed, making sure all sanitizer is rinsed away, then wipe out the inside of the dehydrator.

It is very important that everything is spotless and clean.

Load the dehydrator to capacity, using the product guidelines on thickness and size.

Close the front door, set temperature, fan speed and length of cycle according to product guidelines. Press start.

When the cycle is finished, empty the product and store accordingly.

Clean and prepare the dehydrator for the next cycle.

**Operating the bandsaw/grinder**

When operating a bandsaw or grinder, there must be no disturbances to provide the safest surrounding possible. Before beginning, radio to the store and make them aware that you will be cutting/grinding and give an estimate of how long you will be. Be sure the second warehouse worker is aware and available to receive or load trucks as they come.

Secondly, hang one of the provided laminated signs on the door so that no one will enter, provide a disturbance and contribute to an accident.

When the cutting or grinding is complete, radio to the store to let them know you are finished, notify the second worker as well and remove the sign from the door.

Signed:

Name (print) Title Signature Date

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |