All equipment must have an annual inspection.

Inspections must be completed by the end of the week and mist be dated for that piece of equipment on the annual inspections schedule.

No Holidays when safeties are scheduled unless done prior or the safety is rescheduled. Annual Vehicle In Op. Report is to be filled out.

Highway equipment is to be inspected and any repairs done before going to Turnez Garage for sticker.

All wheels are to be pulled and breaks/bearings are to be inspected unless done less than 3 months prior.

Signed:

Name (print) Title Signature Date

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |